( TL19E00K722000R7101FAAT00 )

DTC Troubleshooting: 71-01, 71-02, 71-03

1. On the sensor side, measure the resistance between following terminals of EPS motor angle sensor 6P connector.

Is the resistance between R1-R2 5−50 Ω, S1-S3 10−100 Ω, and S2-S4 10−100 Ω?

YES | - | Open, or short to body ground in the wire between the EPS motor angle sensor 6P connector and the EPS control unit.■
NO | - | Faulty EPS motor angle sensor (internal failure), or short to body ground in the wire (sensor side), replace the steering gearbox. ■