( TL19E20A18223800000KAAT00 )

Engine Removal

Special Tools Required
Engine tilt hanger set
07KAK-SJ40101
Engine hanger stay
07KAK-SJ40200
Sub hanger stay
07MAK-PY30100
These tools use only for except EU models.
NOTE:

- Use fender covers to avoid damaging painted surfaces.
- To avoid damaging the wiring and terminals, unplug the wiring connectors carefully while holding the connector portion.
- Mark all wiring and hoses to avoid misconnection. Also, be sure that they do not contact other wiring or hoses, or interfere with other parts.

1. Secure the hood in the wide open position (support rod in the lower hole).

1. Relieve fuel pressure.

1. Do the battery removal procedure.

1. Remove the air cleaner housing assembly.

1. Remove the strut brace.