( TL19E00J34600000000CAAT00 )

Combination Light Switch
The driver's MICU controls the lighting system based upon the input signals from each combination light switch.

| Input | Output
--- | --- | ---
Driver's MICU | Combination light switch (OFF) Combination light switch (ON) Combination light switch (POSITION) Combination light switch (PASSING) Combination light switch (DIMMER) | Position light Headlight (high beam, low beam passing) Taillights Headlight (Back-up) to passenger's MICU
B-CAN |  | Position light signal Headlight (high beam, low beam, passing) signals