( TL19E00J26220257121KDAT00 )

Dashboard/Steering Hanger Beam Removal/Installation

1. From under the dash, disconnect the passenger's door wire harness connector (A), the right side wire harness connector(s) (LHD model)/the left side wire harness connectors (B) (RHD model), and the right engine compartment wire harness connectors (LHD model)/the left engine compartment wire harness connectors (RHD model) (C). Disconnect the dashboard wire harness connectors (D) and the audio wire harness connector (E) from the passenger's under-dash fuse/relay box (F). On RHD model, detach the harness clip (G).

1. Detach all of the harness and the connector clips.

LHD model
RHD model