( TL19E1AE34150439533KBAT00 )

M/T Clutch Housing Mainshaft Bearing and Oil Seal Replacement

Special Tools Required
Oil seal driver, 65 mm
07JAD-PL90100
Adjustable bearing puller, 20−40 mm
07JAC-PH80100
Bearing remover shaft
07JAC-PH80200
Bearing driver attachment, 42 x 47 mm
07746-0010300
Driver handle, 15 x 135L
07749-0010000
Slide hammer weight
07741-0010201

1. Remove the ball bearing (A) from the clutch housing (B) using the 20−40 mm adjustable bearing puller (C), slide hammer weight (D) and bearing remover shaft (E).

1. Remove the oil seal (A) from the clutch housing. Be careful when removing the oil seal so the clutch housing is not damaged.

1. Drive in the new oil seal from the transmission side using the 15 x 135L driver handle (A) and 42 x 47 mm bearing driver attachment (B).

1. Drive in the new ball bearing (A) from the transmission side using the 65 mm oil seal driver (B).