( TL19E00J54300065001KBAT00 )

Washer Reservoir Replacement

1. Remove the front bamper.

1. Disconnect the 2P connector(s) (A) from the washer motor(s) (B).

   Washer Reservoir Capacity:
   4.5 L (4.8 US qt, 4.0 Imp qt): | KE, KG, KQ, KN (Without headlight washer) models
   5.0 L (5.3 US qt, 4.4 Imp qt): | KE, KG, KQ, KR (With headlight washer) models

1. Disconnect the washer tube(s) (C), then if necessary, remove the washer motor from the reservoir.
   NOTE: Fluid may flow out of the opening.

1. Remove the clip (A) and three bolts from the washer reservoir (B), then remove the reservoir.

1. Install the washer reservoir in the reverse order of removal. Check the washer motor(s) operation.