( TL19E1PE10411619611KBAT00 )

A/T Differential Carrier Bearing Replacement

Special Tools Required
Installer attachment 40 mm
07LAD-PW50601
NOTE:

- The bearing and the bearing outer race should be replaced as a set.
- Inspect and adjust the carrier bearing preload whenever bearing is replaced.
- Check the bearing for wear and rough rotation. If the bearing is OK, removal is not necessary.

1. Remove the carrier bearing (A) using a commercially available puller (B), a bearing separator (C), and a shaft protector (D).

1. Install new carrier bearings using the 40 mm installer attachment with the small end and a press until it bottoms. Press the carrier bearing on securely so there is no clearance between the carrier bearing and the differential carrier.