( TL19E00J26220219371KDAT20 )

Dashboard Passenger's Undercover Removal/Installation

NOTE:

- Take care not to scratch the dashboard and its related parts.
- When removing components, use the trim tools or equivalent.

1. Remove the Passenger's dashboard undercover (A).

   -1. | Gently pull down the rear edge to detach the clips.
   -2. | Pull the undercover away to release the pins (B) from the holders (C).
   -3. | Disconnect the footwell light connector (D), and if equipped, the HFT control unit connector (E).

1. Install the undercover in the reverse order of removal, and note these items:
   - If the clips are damaged or stress-whitened, replace them with new ones.
   - Push the clips into place securely.
   - Make sure each connector is plugged in properly.
   - Make sure the pins of the undercover are installed securely to the holders.