( TL19E00J32134957891KBAT00 )

Suspension Stroke Sensor Replacement

1. Raise the vehicle, make sure it is securely supported.

1. Disconnect the 3P connector (A) and EPS ground cable (B) from the suspension stroke sensor (C).

1. Remove the bolt and nut, then remove the suspension stroke sensor.

1. Install the sensor in the reverse order of removal.

1. After installing, do the headlight initial position learning.

Front
Rear