( TL19E00J26220219326KDAT00 )

Dashboard Driver's Outer Trim Removal/Installation

NOTE:

- Take care not to scratch the dashboard and its related parts.
- When removing components, use the trim tools or equivalent.
- LHD model is shown; RHD model is symmetrical.

1. Remove the driver's dashboard lower cover.

1. Detach the clips, then remove the driver's outer dashboard trim (A).

1. Install the trim in the reverse order of removal, and note these items:
   - If the clips are damaged or stress-whitened, replace them with new ones.
   - Push the clips into place securely.