( TL19E00J26273413801KDAT00 )

Interior Trim Removal/Installation - Pillar Areas

1. If the side curtain airbag has not been deployed, check the front pillar trim (A) and note the following:
   - To prevent the side curtain airbags from deploying improperly and possibly causing injury, inspect the front pillar trim and replace it if it has any of these types of damage:

   - | Any cracks, deformations, or stress-whitened areas in the front pillar trim
   - | Any cracks or stress-whitened areas in the clip seating surfaces (B)

   - Remove the grommet (C) from the pin (D), and discard the grommet because it was damaged during removal.
   - Replace the grommet with a new one.
   - Do not install the grommet to the pin before checking the overlap between the headliner and the front pillar trim.
   - If the clip (E) is damaged or stress-whitened, replace it with a new one.