( TL19E20A18300043401KCAT00 )

Engine Oil Pan Installation

1. Remove the all of the old liquid gasket from the oil pan mating surfaces, the bolts, and the bolt holes.

1. Clean and dry the oil pan mating surfaces.

1. Apply liquid gasket (P/N 08C70-K0234M, 08C70-K0334M, or 08C70-X0331S) to the engine block mating surface of the oil pan and to the inner threads of the bolt holes.
   NOTE:
   - Apply liquid gasket about 2.5 mm (0.098 in.) diameter bead along the broken line (A).
   - Do not install components if 5 minutes or more have passed after applying the liquid gasket. Instead, remove the old residue and reapply the liquid gasket.