( TL19E20A20326428302FAAT00 )

Fuel Pump Circuit Troubleshooting

1. Turn the ignition switch to ON (II), and measure the voltage between driver's under-dash fuse/relay box connector F (33P) terminal No. 22 and body ground after 2 seconds.

Is there battery voltage?

YES | - | Go to Step 32 .
NO | - | If needed, replace the driver's under-dash fuse/relay box, then go to Step 32 .

1. Turn the ignition switch to LOCK (0).

1. Remove the rear seat cushion.

1. Remove the access panel from the floor.