( TL19E20A14674317531KDAT00 )

Crankshaft Pulley Removal and Installation

1. Install the crankshaft pulley, and hold the pulley with the handle (A) and the crankshaft pulley holder (B).

1. Tighten the bolt to 69 N·m (7.0 kgf·m, 51 lbf·ft) with a torque wrench and 19 x 90L socket (C). Do not use an impact wrench.

1. Tighten the pulley bolt an additional 90 °.

1. Install the drive belt.

1. Install the splash shield.

1. Install the right front wheel.