( TL19E00H46400055413KBAT00 )

Side Impact Sensor (Second) Replacement

Installation

1. Install the side impact sensor (second) with a new TORX bolt (A) then connect the SRS floor wire harness 2P connector (B) to the side impact sensor (second).

1. Reconnect the appropriate side curtain airbag 2P connector.

1. Do the battery terminal reconnection procedure.

1. Confirm proper SRS operation: Turn the ignition switch to ON (II); the SRS indicator should come on for about 6 seconds and then go off.

1. Reinstall all removed parts.