( TL19E30A14666351511MFAT00 )

Cylinder Head Rocker Arm and Shaft Disassembly/Reassembly

NOTE:

- Identify each part as it is removed so that each item can be reinstalled in its original position.
- Inspect the rocker arm shaft and the rocker arms.
- If reused, the rocker arms must be installed in their original location.
- When removing, or installing the rocker arm assembly, do not remove the camshaft holder bolts. The bolts will keep the holders and the rocker arms on the shaft.
- Prior to reassembling, clean all the parts in solvent, dry them, and apply lubricant to any contact points.
- Bundle the intake rocker arms with rubber bands to keep them together as a set.
- When replacing the intake rocker arm assembly, remove the fastening hardware from the new intake rocker arm assembly.

NOTE:

- Identify each part as it is removed so that each item can be reinstalled in its original position.
- Inspect the rocker arm shaft and the rocker arms.
- If reused, the rocker arms must be installed in their original location.
- When removing, or installing the rocker arm assembly, do not remove the camshaft holder bolts. The bolts will keep the holders and the rocker arms on the shaft.
- Prior to reassembling, clean all the parts in solvent, dry them, and apply lubricant to any contact points.
- Bundle the intake rocker arms with rubber bands to keep them together as a set.
- When replacing the intake rocker arm assembly, remove the fastening hardware from the new intake rocker arm assembly.