( TL19E1PE10410800000CAAT20 )

Hydraulic Flow (cont'd)
Shifting between 2nd gear and 3rd gear in D and S with automatic shift mode
As the speed of the vehicle reaches the programmed value, the PCM turns shift solenoid valves C ON, and A and E remain OFF, and B and D remain ON. Shift solenoid valve C pressure (SC) is applied to the right side of shift valve C. Shift valve C is moved to the left side uncovering the A/T clutch pressure control solenoid valve pressure ports leading to the 2nd and 3rd clutches. The PCM controls the A/T clutch pressure control solenoid valves to regulate hydraulic pressure. A/T clutch pressure control solenoid valve B pressure (56) changes to 2nd clutch pressure (20) at shift valve A, and A/T clutch pressure control solenoid valve C pressure (57) changes to 3rd clutch pressure (30) at shift valve A. The 2nd and 3rd clutches are engaged gently.
NOTE: When used, ‘‘left'' or ‘‘right'' indicates direction on the hydraulic circuit.
Driving in 3rd gear in D and S with automatic shift mode
The PCM turns shift solenoid valves B and D OFF, and A and E remain OFF, and C remains ON. Shift solenoid valve B pressure (SB) in the right side of shift valve B is released, and shift valve B is moved to the right side. Shift solenoid valve D pressure (SD) in the left side of shift valve D is released, and shift valve D is moved to the left side. This valve movement switches A/T clutch pressure control solenoid valve C pressure port leading to the 3rd clutch.
A/T clutch pressure control solenoid valve C pressure (57) changes to (5J) at shift solenoid valve D and to (5K) at shift valve B, and becomes 3rd clutch pressure (30) at shift valve A. 3rd clutch pressure (30) is applied to the 3rd clutch, and the 3rd clutch is engaged securely.
NOTE: When used, ‘‘left'' or ‘‘right'' indicates direction on the hydraulic circuit.