( TL19E00J4616185367CKBAT00 )

Front Seat Up-down Motor Motor Replacement

1. Install the rear brake mounting bolts (A), and using a TORX T30 bit, secure them to their specified torque. Using TORX T40 and T30 bits, fasten the rear brake bracket mounting bolts (B, C) to their specified torque.

1. Reinstall all of removed parts to the seat frame:
   - Seat-back cover/pad
   - Seat cushion cover/pad

1. Reinstall the front seat.

1. Check the front seat up-down operation.