( TL19E00J26273450001KDAT00 )

Interior Trim Removal/Installation - Rear Shelf Area

Rear Shelf
SRS components are located in this area. Review the SRS component locations and the precautions and procedures before doing repairs or service.
NOTE:

- Put on gloves to protect your hands.
- Take care not to bend or scratch the rear shelf, rear bulkhead cover, and the trim.
- When removing components, use the trim tools or equivalent.

1. Remove these items:
   - Rear seat cushion
   - Rear seat side bolster, both sides
   - Rear door opening seal, as needed
   - Rear pillar trim, both sides
   - Rear center seat belt lower anchor

1. Fold both the rear seat-backs forward.

1. If both the rear bulkhead cover and the rear shelf are to be removed from the trunk compartment, turn the high mount brake light socket (A) 45 ° counterclockwise to remove the socket.