( TL19E20A20326428001KCAT00 )

Fuel Line/Quick-Connect Fitting Installation

1. Insert a new retainer (A) into the connector (B) if the retainer is damaged, or after:
   - replacing the fuel rail.
   - replacing the fuel line.
   - replacing the fuel pump.
   - replacing the fuel filter.
   - replacing the fuel tank.
   - removing the retainer from the line.
   - Use the same manufacturer retainer and the same size retainer when the replacing the retainer.