( TL19E1PE10411310041LDAT00 )

A/T 1st, 2nd, and 3rd Clutch Reassembly

1. Compress the return spring carefully until the snap ring can be installed. Check the spring retainer (A) is properly installed on the clutch hub (B). If improperly installed, change the position of the spring compressor attachment and the spring retainer.
   NOTE: Insert the spring retainer so it can be adjusted (center of tolerance) to prevent damaging the spring retainer oil seal.