( TL19E00B20200056851KBAT00 )

Front Stabilizer Bar Replacement

1. Raise the front of the vehicle, and support it with safety stands in the proper locations.

1. Remove the front wheels.

1. Disconnect both tie-rod ball joints from the knuckle.

1. Disconnect both stabilizer links from the stabilizer bar.

1. Remove the flange bolts (A) and the bushing holders (B), then remove the bushings (C) and the stabilizer bar (D).
   NOTE: During installation, align the paint marks (E) on the stabilizer bar with the side of the bushings.

1. Install the stabilizer bar.
   NOTE:
   - Note the right and left direction of the stabilizer bar.
   - Note the direction of installation for the bushings and the bushing holders.

1. Install all of the removed parts in the reverse order of removal, and note these items:
   - Refer to stabilizer link removal/installation to connect the stabilizer bar to the links.
   - Before installing the wheel, clean the mating surfaces of the brake disc and inside of the wheel.

1. Check the wheel alignment, and adjust it if necessary.