( TL19E00J26273457073KDAT00 )

Steering Column Cover Removal/Installation

1. Turn the steering wheel to left, and release the left tab (A) of the upper column cover (B) while pushing the lower column cover (C) from the front side.
   Carefully release the tabs, and note the hooks (D) may break when the upper column cover is pulled up too hard.

1. Turn the steering wheel to right, and release the right tab of the upper column cover the same as the Step 3 .