( TL19E00H46200053402KBAT00 )

Rear Seat Belt Replacement

1. Remove the center anchor bolts (A), then remove the right seat belt buckle (B), the center seat belt buckle (C), and the left seat belt buckle (D).

1. Fold the rear seat-backs forward.

1. Pull the center seat belt out through the slit in the seat belt guide.

1. Remove these items:
   - Rear seat side bolsters, both sides
   - Rear door opening seal, as needed
   - Rear pillar trim, both sides
   - Rear bulkhead cover
   - Rear shelf