( TL19E00J46161854027KBAT00 )

Front Seat Recline Motor Replacement

8-way Power Seat
SRS components are located in this area. Review the SRS component locations and the precautions and procedures before doing repairs or service.
NOTE: Put on gloves to protect your hands.

1. Remove the front seat.

1. Remove the seat-back cover and pad.

1. Release the push nut (A) from the motor side end of the connecting rod (B), gently tap on the motor side of the connecting rod to remove it from the recline motor (C) and both recline adjusters (D). The driver's seat on LHD model is shown; the passenger's seat is symmetrical; the ones on RHD model are similar.

1. Remove the bolt, then remove the recline motor (A). The driver's seat on LHD model is shown; the passenger's seat is symmetrical; the ones on RHD model are similar.

1. Install the motor in the reverse order of removal, and note these items:
   - Replace the push nut with a new one. Make sure the push nut is installed correctly.
   - Make sure the recline motor harness is routed properly.
   - Apply medium strength liquid thread lock to the mounting bolt before reinstallation.