( TL19E00J32112513327KBAT00 )

Automatic Lighting/Rain Sensor Replacement

NOTE:

- If the automatic lighting/rain sensor 6P connector is connected after the battery terminal is connected, the automatic lighting/rain sensor is not confirmed by driver's MICU.
- If the driver's MICU does not confirm the automatic lighting/rain sensor, automatic wiper system does not work.
- Connect the automatic lighting/rain sensor 6P connector first, then connect the battery terminal.

1. Remove the automatic lighting/rain sensor cover (A) and disconnect the 6P connector (B).

1. Remove the lock (C), then remove the automatic lighting/rain sensor (D).

1. Install the automatic lighting/rain sensor in the reverse order of removal.