( TL19E1PE1041141228CKBAT00 )

A/T Shift Lever Boot and A/T Gear Position Indicator Panel Base Replacement

1. Remove the shift lever assembly.

1. Remove the shift lever knob.

1. Remove the A/T gear position indicator panel light socket (A) from the indicator panel base (B).

1. Remove the A/T gear position indicator panel base from the shift lever bracket (C).

1. Remove the A/T gear position indicator panel (A), from the panel base (B).

1. Release the lock tabs (A) retaining the shift lever boot (B) using a screwdriver.

1. Replace the shift lever boot (A) or the A/T gear position indicator panel base (B).

1. Install the shift lever boot on the indicator panel base.

1. Install the A/T gear position indicator panel on the indicator panel base.

1. Install the A/T gear position indicator panel base (A) on the shift lever bracket (B).
   NOTE: Take care not to pinch the harness.

1. Install the A/T gear position indicator panel light socket (C) in the indicator panel base.

1. For LHD model: Route the A/T gear position indicator panel light harness. Take a slack out of the harness, and secure the harness with at the guide.

1. Install the shift lever knob.

1. Install the shift lever assembly.