( TL19E30A14400049001NAAT00 )

Radiator

Item | Measurement | Qualification | Standard or New
--- | --- | --- | ---
Radiator | Coolant capacities (including engine, heater, hoses, and reservoir) Use genuine Honda All Season Antifreeze/Coolant Type 2 (except KQ) | A/T: engine overhaul | 8.6 L (2.27 US gal, 1.89 Imp gal)
A/T: coolant change | 6.5 L (1.71 US gal, 1.42 Imp gal)
M/T: engine overhaul | 8.7 L (2.30 US gal, 1.91 Imp gal)
M/T: coolant change | 6.6 L (1.74 US gal, 1.45 Imp gal)
Coolant capacities (including engine, heater, hoses, and reservoir) Use genuine Honda All Season Antifreeze/Coolant Type 2 (KQ) | A/T: engine overhaul | 8.2 L (2.16 US gal, 1.80 Imp gal)
A/T: coolant change | 6.1 L (1.61 US gal, 1.34 Imp gal)
M/T: engine overhaul | 8.3 L (2.19 US gal, 1.83 Imp gal)
M/T: coolant change | 6.2 L (1.63 US gal, 1.36 Imp gal)