( TL19E00J20100065311KBAT00 )

Rear Wheelhouse Gusset Replacement

NOTE:

- Put on gloves to protect your hands.
- Take care not to scratch the body and related parts.

1. Remove these items:
   - Rear seat-back
   - Rear seat cushion
   - Rear seat side bolster
   - Trunk side trim panel:

   - | With temporary repair kit (TRK)/with compact spare tyre
   - | With normal spare tyre

   - Rear wheelhouse insulator

1. Remove the bolts (A), then remove the rear wheelhouse gusset (B).

1. Install the gusset in the reverse order of removal.