( TL19E00K791000R921XFAAT00 )

DTC Troubleshooting: 92-1x

DTC 92-1x (‘‘x'' can be 0 thru 9 or A thru F):
Short to Power in the Passenger's Airbag Off Indicator
NOTE:

- Before doing this troubleshooting procedure, review SRS Precautions and Procedures and General Troubleshooting Information.
- Troubleshoot DTC A1-1x before doing this troubleshooting procedure.
- Before replacing the SRS unit, check the SRS unit software version with the HDS. If the software version is not the latest, update the SRS unit software and retest.

1. Clear the DTC memory.

1. Turn the ignition switch to ON (II), then wait for 10 seconds.

1. Read the DTC.

Is DTC 92-1x indicated?

YES | - | Go to Step 4 .
NO | - | Intermittent failure, the system is OK at this time. Go to Troubleshooting Intermittent Failures. If another DTC is indicated, troubleshoot the DTC.

1. Disconnect the passenger's airbag off indicator 6P connector.

1. Turn the ignition switch to LOCK (0).

1. Do the battery terminal disconnection procedure , then wait for 3 minutes.

1. Disconnect SRS unit connector A (39P) from the SRS unit.

1. Do the battery terminal reconnection procedure.

1. Turn the ignition switch to ON (II).

1. Measure the voltage between the No. 20 terminal of SRS unit connector A (39P) and body ground. There should be less than 0.5 V.

Is the voltage as specified?

YES | - | Faulty SRS unit or passenger's airbag off indicator; replace the passenger's airbag off indicator. If the problem is still present, replace the SRS unit. ■
NO | - | Short to power in the dashboard wire harness or the audio wire harness; replace the faulty harness.■