( TL19E00E16226600000LCAT00 )

Driveshaft Disassembly

1. Make marks (A) on the rollers (B) and the spider (C) to identify the locations of the rollers on the spider, then remove the rollers.
   NOTE: Do not engrave or scribe any marks on the rolling surface.

1. Remove the circlip (D).

1. Make marks (E) on the spider and driveshaft (F) to identify the position of the spider on the shaft.

1. Remove the spider.
   NOTE: If necessary, use a commercially available puller.