( TL19E30A14666300000KCAT00 )

Cylinder Head Rocker Arm Assembly Installation

1. Reassemble the rocker arm assembly.

1. Clean and dry the No. 5 rocker shaft holder mating surface.

1. Apply liquid gasket (P/N 08C70-K0234M, 08C70-K0334M, or 08C70-X0331S) to the cylinder head mating surface of the No. 5 rocker shaft holder.
   NOTE:
   - Apply liquid gasket about 3 mm (0.12 in.) diameter bead along the broken line (A).
   - Do not install components if 5 minutes or more have passed after applying the liquid gasket. Instead, remove the old residue and reapply the liquid gasket.

1. Insert the bolts (A) into the rocker shaft holder, then install the rocker arm assembly (B) on the cylinder head.

1. Remove the bolts from the rocker shaft holder.

1. Make sure the punch marks on the variable valve timing control (VTC) actuator and the exhaust camshaft sprocket are facing up, then set the camshafts (A) in the holder.

1. Set the camshaft holders (B) and cam chain guide B (C) in place.

1. Tighten the bolts to the specified torque.
   NOTE: If the engine does not have bolt (21), skip it and continue the torque sequence.

   Specified Torque
   8 x 1.25 mm 22 N·m (2.2 kgf·m, 16 lbf·ft)
   6 x 1.0 mm 12 N·m (1.2 kgf·m, 8.8 lbf·ft)
   6 x 1.0 mm Bolts: (21), (22), (23)

1. Install the cam chain, then adjust the valve clearance.