( TL19E00F18100000000FAAT02 )

EPS Symptom Troubleshooting - EPS indicator does not go off, and no DTCs are stored

1. Check for continuity between EPS control unit connector D (28P) terminal No. 15 and gauge control module 32P connector terminal No. 21.

Is there continuity?

YES | - | Check for loose terminals in the EPS control unit connectors, and repair if necessary. If no poor connections are found, replace the EPS control unit. ■
NO | - | Repair open in the wire between the EPS control unit and the gauge control module.■