( TL19E1AE34150439755MBAT00 )

M/T Clutch Housing Mainshaft Thrust Clearance Adjustment

1. Thoroughly clean the 28 mm spring washer (A) and the 28 mm washer (B) before installing them on the clutch housing side ball bearing (C). Note the installation direction of the spring washer.

1. Assemble the all of mainshaft components correctly: R20A3 engine model, K24Z3 engine model.

1. Install the mainshaft assembly in the clutch housing.

1. Place the transmission housing over the mainshaft and onto the clutch housing.

1. Tighten the clutch and transmission housings with several 8 mm bolts.
   NOTE: It is not necessary to use sealing agent between the housing for this procedure.

1. Lightly tap on the mainshaft with a plastic hammer.