( TL19E00J32134957892FAAT00 )

Suspension Stroke Sensor Circuit Troubleshooting

1. Measure the voltage between the front and rear suspension stroke sensor 3P connector No. 1 terminal and body ground individually.

Is there about 5 V?

YES | - | Go to Step 8 .
NO | - | Check for an open or a short in the wire between the headlight leveling control unit and the front (or rear) suspension stroke sensor. If the wire is OK, replace the front (or rear) suspension stroke sensor.■