( TL19E00H46400000000MDAT00 )

SRS Component Replacement/Inspection After Deployment

NOTE:

- Before doing any SRS repairs, check the DTCs, for the less obvious deployed components (seat belt tensioners, front impact sensors, side airbag sensors, etc.).
- Do not replace the OPDS unit unless it is physically damaged or a specific fault was found during DTC troubleshooting.
- After a vehicle collision, inspect the front seat active head restrains.

After a collision where the seat belt tensioners deployed, replace these items:

- SRS unit
- Seat belt tensioners
- Front impact sensors

After a collision where the front airbag(s) deployed, replace these items:

- SRS unit
- Deployed airbag(s)
- Seat belt tensioners
- Front impact sensors

After a collision where the side airbag(s) deployed, replace these items:

- SRS unit
- Deployed side airbag(s)
- Side impact sensor(s) (first) for the side(s) that deployed
- Side impact sensor(s) (second) for the side(s) that deployed
- Center pillar lower trim
- Complete seat frame

After a collision where a side curtain airbag has deployed, replace the items for the side(s) that deployed:

- SRS unit
- Deployed side curtain airbag(s)
- Seat belt tensioner(s) for the side(s) that deployed
- Side impact sensor(s) (first) for the side(s) that deployed
- Side impact sensor(s) (second) for the side(s) that deployed
- Rear safing sensor
- Roof trim
- Front pillar trim
- Center pillar upper trim
- Rear pillar trim
- Front grab handle
- Rear grab handle
- All related trim clips
- Sunvisor

After a moderate to severe side or rear collision, inspect for any damage on the side curtain airbag or other related components. Replace the components as needed.
During the repair process, inspect these areas:

- Inspect all the SRS wire harnesses. Replace, do not repair, any damaged harnesses.
- Inspect the cable reel for heat damage. If there is any damage, replace the cable reel.

After the vehicle is completely repaired, turn the ignition switch to ON (II). If the SRS indicator comes on for about 6 seconds and then goes off, the SRS is OK. If the indicator does not function properly, use the HDS to read the DTC. If you cannot retrieve a code, do the SRS Symptom Troubleshooting.

Front pillar trim
Center pillar trim
Rear pillar trim

Checking and Adjusting the Headliner/Pillar Trim Overlap
To prevent the side curtain airbag from deploying and damaging the pillar trim, the overlap between the headliner and pillar trim must be less then 8 mm (0.3 in.). To check the overlap, do this:

1. Install the headliner (A) and the pillar trim (B).

1. Using masking tape on the headliner, mark the upper edge of each pillar trim.

1. Remove the pillar trim, and measure the headliner overlap.
   - If the overlap is less than 8 mm (0.3 in.), remove the tape, and install the pillar trim.
   - If the overlap is more than 8 mm (0.3 in.), go to Step 4 .

1. Carefully trim the headliner with a utility knife, reducing the overlap to less than 8 mm (0.3 in.).

1. Remove the tape, and install the pillar trim.