( TL19E1PE10480139301KCAT00 )

A/T Valve Body and ATF Strainer Installation

Exploded View
NOTE: Refer to the Exploded View as needed during the following procedures.

1. Make sure that the ATF magnet is clean and installed in the torque converter housing.

1. Install the main separator plate (A) and the two dowel pins on the torque converter housing. Then install the ATF pump drive gear (B), the ATF pump driven gear (C), and the ATF pump driven gear shaft (D). Lubricate all parts with ATF, and install the ATF pump driven gear with its grooved and chamfered side facing down.

1. Install the main valve body.