( TL19E00K77C000Y2629FAAT00 )

DTC Troubleshooting: B2629

DTC B2629:
Left Rear Corner Parking Sensor Malfunction

1. Clear the DTCs with the HDS.

1. Turn the ignition switch to LOCK (0) and then back to ON (II).

1. Check for DTCs with the HDS.

Is DTC B2629 indicated?

YES | - | Go to Step 4 .
NO | - | Intermittent failure, the system is OK at this time.■

1. Turn the ignition switch to LOCK (0).

1. Swap the left rear corner parking sensor and the left rear center parking sensor.

1. Turn the ignition switch to ON (II).

1. Check for DTCs with the HDS.

Is DTC B2629 indicated?

YES | - | Go to Step 8 .
NO | - | Replace the left rear corner parking sensor.■

1. Turn the ignition switch to LOCK (0).

1. Disconnect the 6P connector from the left rear corner parking sensor.

1. Turn the ignition switch to ON (II).

1. Measure the voltage between the left rear corner parking sensor 6P connector No. 6 terminal and body ground.

Is there about 8 V?

YES | - | Go to Step 12 .
NO | - | Go to Step 22 .

1. Turn the ignition switch to LOCK (0).