( TL19E00H46200053401KBAT00 )

Front Seat Belt Replacement

1. Remove the center anchor bolt (A), and detach the harness clips (B), then remove the seat belt buckle (C).
   NOTE: The driver's seats on LHD model are shown; the passenger's seats on LHD model are symmetrical. Both front seats on RHD model are similar.

1. Manual seat: Release the hook strip (D), and pull back the seat cushion cover.

1. Pull the seat belt switch harness (E) out through the space between the seat cushion and the seat track.

Driver's seat/passenger's seat (8-way power seat)
Driver's seat (manual height adjustable seat)
Driver's seat/passenger's seat (manual seat)