( TL19E000000000J0214NDAT00 )

Steering

Item | Measurement | Qualification | Standard or New
--- | --- | --- | ---
Steering wheel | Rotational play measured at outside edge with engine running |  | 0−10 mm (0−0.39 in.)
Initial turning load measured at outside edge with engine running |  | 29 N (3.0 kgf, 6.6 lbf)
Gearbox | Angle of rack guide screw loosened from locked position |  | 10±5 °

Suspension

Item | Measurement | Qualification | Standard or New | Service Limit
--- | --- | --- | --- | ---
Wheel alignment | Camber | 16 inch wheel | Front | 0 °02 '±30 '
Rear | −0 °50 '±30 '
17 inch wheel | Front | 0 °00 '±30 '
Rear | −1 °00 '±30 '
18 inch wheel | Front | 0 °03 '±30 '
Rear | −1 °12 '±30 '
Caster | 16 inch wheel | Front | 3 °43 ' +10 ' −50 '
17 inch wheel | Front | 3 °47 ' +10 ' −50 '
18 inch wheel | Front | 3 °52 ' +10 ' −50 '
Total toe-in | Front | 0±2 mm (0±0.08 in.)
Rear | 2±2 mm (0.08±0.08 in.)
Front wheel turning angle | 16 inch wheel | Inward | 39 °04 '±2 °
Outward (reference) | 31 °33 '
17 inch wheel | Inward | 38 °58 '±2 °
Outward (reference) | 31 °28 '
18 inch wheel | Inward | 36 °59 '±2 °
Outward (reference) | 30 °23 '
Wheel | Steel wheel runout | Axial | 0−1.0 mm (0−0.04 in.) | 2.0 mm (0.08 in.)
Radial | 0−1.0 mm (0−0.04 in.) | 1.5 mm (0.06 in.)
Aluminium wheel runout | Axial | 0−0.7 mm (0−0.03 in.) | 2.0 mm (0.08 in.)
Radial | 0−0.7 mm (0−0.03 in.) | 1.5 mm (0.06 in.)
Wheel bearing | End play | Front | 0−0.05 mm (0−0.002 in.)
Rear | 0−0.05 mm (0−0.002 in.)

Brakes

Item | Measurement | Qualification | Standard or New | Service Limit
--- | --- | --- | --- | ---
Parking brake | Distance traveled when lever pulled with 196 N (20 kgf, 44 lbf) of force | Rear disc brake | 6 to 8 clicks
Rear drum in disc brake | 5 to 7 clicks
Drum I.D. (rear drum in disc brake) |  | 189.9−190.0 mm (7.476−7.480 in.) | 191.0 mm (7.520 in.)
Shoe lining thickness (rear drum in disc brake) |  | 3.4 mm (0.133 in.) | 1.0 mm (0.04 in.)
Brake pedal | Pedal height (carpet moved aside) | LHD | M/T | 164 mm (6.46 in.)
A/T | 173 mm (6.81 in.)
RHD | M/T | 167 mm (6.57 in.)
A/T | 172 mm (6.77 in.)
Free play |  | 1−5 mm (0.04−0.20 in.)
Brake disc | Thickness | Front | 1-piston caliper | 24.9−25.1 mm (0.98−0.99 in.) | 23.0 mm (0.91 in.)
2-piston caliper | 31.9−32.1 mm (1.255−1.263 in.) | 30.0 mm (1.18 in.)
Rear |  | 8.9−9.1 mm (0.35−0.36 in.) | 8.0 mm (0.31 in.)
Runout | Front and rear | ——— | 0.04 mm (0.0016 in.)
Parallelism | Front and rear | ——— | 0.015 mm (0.0006 in.)
Brake pads | Thickness | Front | 1-piston caliper | 10.5−11.0 mm (0.41−0.43 in.) | 1.5 mm (0.059 in.)
2-piston caliper | 10.5−11.0 mm (0.41−0.43 in.) | 1.6 mm (0.063 in.)
Rear |  | 8.3−9.0 mm (0.33−0.35 in.) | 1.0 mm (0.04 in.)
Brake booster | Master cylinder oil pressure | Except KQ | VacuumkPa (mmHg, in.Hg) | Brake pedal pressure N (kgf, lbf) | kPa (kgf/cm 2 , psi)
0 (0, 0) | 98 (10, 22) | 0 (0, 0)
294 (30, 66) | 1,539 (15.7, 223)
66.7 (500, 19.7) | 98 (10, 22) | 4,988 (50.9, 723)
294 (30, 66) | 9,055 (92.3, 1,313)
KQ | Vacuum kPa (mmHg, in.Hg) | Brake pedal pressure N (kgf, lbf) | kPa (kgf/cm 2 , psi)
0 (0, 0) | 98 (10, 22) | 0 (0, 0)
294 (30, 66) | 1,754 (17.9, 254)
66.7 (500, 19.7) | 98 (10, 22) | 6,399 (65.3, 928)
294 (30, 66) | 11,809 (120.4, 1,713)

Air Conditioning

Item | Measurement | Qualification | Standard or New
--- | --- | --- | ---
Refrigerant | Type |  | HFC-134a (R-134a)
Capacity of system |  | 450−500 g (15.9−17.7 oz)
Refrigerant oil | Type |  | SP-10 (P/N 38897-P13-A01AH or 38899-P13-A01)
Capacity of components | Condenser | 50 mL (1 2/3 fl·oz, 1.8 Imp oz)
Evaporator | 40 mL (1 1/3 fl·oz, 1.6 Imp oz)
Each line and hose | 10 mL (1/3 fl·oz, 0.4 Imp oz)
Receiver/Dryer | 10 mL (1/3 fl·oz, 0.4 Imp oz)
Compressor (Except KQ) | 80−90 mL (2 5/7−3 fl·oz, 2.6−3.0 Imp oz)
Compressor (KQ) | 75−85 mL (2 1/2−2 5/6 fl·oz, 2.6−3.0 Imp oz)
Compressor | Field coil resistance |  | 3.15−3.45 Ω
Pulley-to-armature plate clearance |  | 0.35−0.65 mm (0.014−0.026 in.)