( TL19E00R51100000000YDAT03 )

Cross Section of Body and Sealants - General

NOTE: Follow the sealer manufacturer's instructions, and apply the sealer. Note the following items:

- Clean the areas to be sealed with wax and grease remover.

- Wipe off any excess spot sealer with thinner. After the primer is sprayed, sealer will fill the area where the spot sealer was wiped.

- Make sure you can see the sealant when the sealed part is in its proper location. For the details, refer to engine compartment and damper housing, damper housing and dashboard upper, front wheelhouse and front side frame, dashboard upper, dashboard lower, and front floor, middle floor, rear floor and spare tyre pan/roof panel, rear side outer panel and rear panel, and rear wheelhouse.

- When applying sealant to the engine compartment, the door opening, and the trunk lid gutter, try to match the appearance of the factory sealer. Wipe off any excess sealer.

- Apply sealer to any area that a replacement part will cover. Smooth the sealer with a brush if necessary.