( TL19E30A20326428201KBAT00 )

Fuel Pressure Regulator Replacement

1. Remove the fuel tank unit.

1. Remove the reservoir (A).

1. Remove the bracket (B).

1. Remove the fuel pressure regulator (C).

1. Install the parts in the reverse order of removal with new O-rings (D) and a new bracket. When installing the fuel tank unit, align the marks on the unit and the fuel tank.
   NOTE:
   - Coat the O-rings with clean engine oil; do not use any other oils or fluids.
   - Use all supplied new parts in the pressure regulator replacement kit.
   - Do not pinch the O-rings during installation.