( TL19E00J32300063101FHAT00 )

Vanity Mirror Light Test/Replacement

1. Remove the sunvisor.

1. Disconnect the 2P connector (A) from the sunvisor (B).

   Vanity Mirror Light: | 2 W x 2

1. Check for continuity between the No. 1 and No. 2 terminals.
   - With the vanity mirror cover (C) opened, there should be continuity.
   - With the vanity mirror cover closed, there should be no continuity.

1. If the continuity is not as specified, check the bulbs (D). If the bulbs are OK, replace the vanity mirror light.