( TL19E20A18316600000MAAT90 )

Crankshaft Inspection

Straightness

1. Place the engine block on a flat surface, crankshaft side up plate.

1. Clean and install the bearings on the No. 1 and the No. 5 journals of the engine block.

1. Lower the crankshaft into the engine block.

1. Measure the runout on all of the main journals. Rotate the crankshaft two complete revolutions. The difference between measurements on each journal must not be more than the service limit.
   Crankshaft Total Runout

   Standard (New): | 0.03 mm (0.0012 in.) max.
   Service Limit: | 0.04 mm (0.0016 in.)