( TL19E30A14680851519KDAT00 )

VTEC Rocker Arm Oil Control Valve Removal/Installation

1. Remove the strut brace.

1. Disconnect the rocker arm oil control solenoid connector (A).

1. Remove the harness clamps (B) and the bolts (C).

1. Remove the rocker arm oil control valve assembly (D) and the rocker arm oil control valve filter (E).

1. Remove the engine wire harness bracket (A), from the rocker arm oil control valve (B).

1. Install the parts in the reverse order of removal with a new rocker arm oil control valve filter.