( TL19E00J26220230115KBAT00 )

Glove Box Lock Cylinder Replacement

NOTE: Take care not to scratch the glove box.

1. Remove the glove box.

1. Lift the glove box handle (A), and use a release one end of the retainer (B) from its slot.
   NOTE:
   - Do not remove the retainer entirely. Leave one end of the retainer in its original position when removing the lock cylinder.
   - LHD model: Use a hook-shaped tool to pull the middle of the retainer.
   - RHD model: Use a flat-tip screwdriver to push out the end of the retainer.

LHD model
RHD model

1. Remove the glove box lock cylinder (A).

1. Reinstall the end of the retainer (A) in its slot, then reinstall the lock cylinder (B). Push the cylinder into place securely until the retainer snaps into place.

LHD model
RHD model