( TL19E1PE10474000000CAAT00 )

Lock-up System (cont'd)
Full Lock-up
When the vehicle speed increases, the PCM commands A/T clutch pressure control solenoid valve A to increase A/T clutch pressure control solenoid valve A pressure (55), and the lock-up control valve is moved to the left by the increased pressure. Then torque converter pressure (94) from the left side of the torque converter is completely released at the lock-up control valve, and torque converter pressure (91) engages the torque converter clutch securely; the torque converter clutch is in full lock-up.
NOTE: When used, ‘‘left'' or ‘‘right'' indicates direction on the hydraulic circuit.