( TL19E00K70900081300FAAT00 )

DTC Troubleshooting: 30

1. Check for voltage between the relay circuit board 10P connector No. 5 terminal and body ground.

Is there battery voltage?

YES | - | Go to Step 25 .
NO | - | Repair an open in the wire between the No. 6 (7.5 A) fuse in the driver's under-dash fuse/relay box and relay circuit board.■

1. Turn the ignition switch to LOCK (0).

1. Disconnect the 20P connector from the ACC unit.