( TL19E00K764000Y1147FAAT00 )

DTC Troubleshooting: B1147

DTC B1147:
Left Rear Power Window Position Information Error

1. Clear the DTC with the HDS.

1. Turn the ignition switch to LOCK (0) and then back to ON (II).

1. Open and close the left rear power window by using the left rear power window switch manually.

1. Check for DTCs with the HDS.

Is DTC B1147 indicated?

YES | - | Go to Step 5 .
NO | - | Intermittent failure, the system is OK at this time. Check for loose or poor connections.■

1. Check for DTCs with the HDS.

Is DTC B1132 and B1133 indicated?

YES | - | Troubleshoot the indicated DTC(s) first.■
NO | - | Reset the left rear power window, and recheck.