( TL19E00K75100081060FAAT00 )

DTC Troubleshooting: 6

1. Check for continuity between LKAS control unit 26P connector No. 25 terminal and ECM/PCM connector A (49P) No. 4 terminal.

Is there continuity?

YES | - | The F-CAN line is OK at this time. Check for loose terminals in the LKAS control unit connector, and repair if necessary. If all connections are OK, replace the LKAS control unit. ■
NO | - | Repair an open in the wire between the LKAS control unit and the branch of the F-CAN line (CANL).■